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	BUILDING / SITE
	
	FLOOR / AREA
	
	MONTH / YEAR
	
	INSPECTOR
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Checks (OSHA 1910.157(e)(2), NFPA 10 ch. 7): in designated place, unobstructed and visible · pressure gauge in operable range · pin in place and tamper seal intact · hose and nozzle clear, no cracks · no corrosion, dents, leaks · fullness by weight or heft · inspection tag and location sign present. Any failed item: remove from service, replace, and record the action.
	
	
	
	
	

	Inspector signature
	
	Reviewed by (safety officer)
	
	Date
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