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	HOME
	
	YEAR
	
	HVAC FILTER SIZE
	
	HANDYMAN / HVAC / PLUMBER

	
	
	
	
	
	
	



	EVERY MONTH
	
	SPRING

	☐  Check / replace HVAC filter
	
	
	☐  Clean gutters and downspouts
	

	☐  Test smoke and CO alarms
	
	
	☐  Inspect roof and flashing
	

	☐  Clean range hood filter
	
	
	☐  Service the air conditioner
	

	☐  Run water in unused sinks
	
	
	☐  Check outside faucets for damage
	

	☐  Check under sinks for leaks
	
	
	☐  Inspect siding, paint and caulk
	

	☐  Clean garbage disposal
	
	
	☐  Clean and repair window screens
	

	
	
	☐  Check sump pump
	

	SUMMER
	
	

	☐  Check deck and fence
	
	
	FALL

	☐  Clean dryer vent duct
	
	
	☐  Clean gutters after leaves fall
	

	☐  Inspect for pests and termites
	
	
	☐  Service furnace or heat pump
	

	☐  Trim plants back from the house
	
	
	☐  Shut off and drain outside faucets
	

	☐  Test garage door auto-reverse
	
	
	☐  Weatherstrip doors and windows
	

	
	
	☐  Chimney inspected and swept
	

	WINTER
	
	☐  Reverse ceiling fans to clockwise
	

	☐  Check attic for ice dams and leaks
	
	
	☐  Test the generator
	

	☐  Heat at 55°F or more when away
	
	
	

	☐  Clear snow from vents and meter
	
	
	

	☐  Flush water heater (once a year)
	
	
	

	☐  Check caulk around tubs
	
	
	

	☐  Test GFCI outlets
	
	
	

	☐  Check fire extinguisher pressure
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